Technology In Action, Complete, 11e (Evans et al.)
Chapter 7  Networking: Connecting Computing Devices

1) A computer ________ is two or more computers connected using software and hardware so that they can communicate with each other. 
A) network
B) switch
C) broadband
D) node
Answer:  A
Diff: 1
Section Ref:  Networking Fundamentals

2) A ________ is a device connected to a network such as a printer or a game console.
A) packet
B) node
C) NOS
D) NIC
Answer:  B
Diff: 1
Section Ref:  Networking Fundamentals

3) ________ is the actual speed of data transfer that is achieved and is always less than or equal to the data transfer rate.
A) Benchmark
B) Broadband
C) Bandwidth
D) Throughput 
Answer:  D
Diff: 2
Section Ref:  Networking Fundamentals

4) All of the following are tasks for network administration of a large organization EXCEPT ________.
A) installing new computers and devices on the network
B) updating and installing new software on the network
C) monitoring network performance
D) purchasing initial equipment for the network
Answer:  D
Diff: 2
Section Ref:  Networking Fundamentals


5) Which of the following is NOT used to classify network architectures?
A) Distance between nodes
B) Communication medium
C) Speed of the network
D) Protocol used to exchange data
Answer:  C
Diff: 3
Section Ref:  Network Architectures
6) ________ is the maximum speed at which data can be transferred between two nodes.
A) Throughput
B) Bandwidth
C) Broadband
D) Through speed
Answer:  B
Diff: 2
Section Ref:  Networking Fundamentals

7) A ________ is a network located in your residence that connects to all your digital devices.
A) MAN
B) WAN
C) HAN
D) LAN
Answer:  C
Diff: 2
Section Ref:  Network Architectures Defined by Distance

8) A network that spans a large physical distance is called a ________.
A) MAN
B) LAN
C) PAN
D) WAN
Answer:  D
Diff: 2
Section Ref:  Network Architectures Defined by Distance

9) A large network designed to provide access to a specific geographic area, such as a large city, is a ________.
A) MAN
B) PAN
C) LAN
D) WAN
Answer:  A
Diff: 2
Section Ref:  Network Architectures Defined by Distance


10) Which transmission medium transmits data the fastest?
A) Twisted-pair cable
B) Coaxial cable
C) Wireless
D) Fiber-optic cable
Answer:  D
Diff: 3
Section Ref:  Transmission Media
11) Normal telephone cable is a type of ________.
A) fiber-optic cable
B) twisted-pair cable
C) coaxial cable
D) Ethernet cable
Answer:  B
Diff: 2
Section Ref:  Transmission Media

12) A client/server network is an example of ________ administration
A) local
B) wide area
C) central
D) remote
Answer:  C
Diff: 2
Section Ref:  Network Architectures Defined by Levels of Administration

13) A peer-to-peer (P2P) network is an example of ________ administration.
A) local
B) wide area
C) central
D) corporate
Answer:  A
Diff: 2
Section Ref:  Network Architectures Defined by Levels of Administration

14) The fastest version of wireless Ethernet is ________.
A) 802.11n
B) 802.11g
C) 802.11ab
D) 802.11ac
Answer:  D
Diff: 3
Section Ref:  Ethernet Protocols


15) Which of the following is NOT a type of cable used in wired networks?
A) Unshielded twisted-pair
B) Coaxial
C) Fiber-optic
D) Unshielded coaxial
Answer:  D
Diff: 3
Section Ref:  Transmission Media
16) Which of the following is NOT a type of UTP cable you would use in a wired Ethernet network?
A) Cat 5E
B) Cat 6
C) Cat 6A
D) Cat 7B
Answer:  D
Diff: 3
Section Ref:  Transmission Media

17) The most popular transmission media option for wired home Ethernet networks is ________ cable.
A) fiber-optic
B) power-line
C) unshielded twisted-pair (UTP)
D) coaxial
Answer:  C
Diff: 2
Section Ref:  Transmission Media

18) Wireless network devices use ________ to communicate with each other.
A) fiber optics
B) satellites
C) radio waves
D) DSL
Answer:  C
Diff: 2
Section Ref:  Transmission Media

19) For the nodes on a network to communicate with each other and access the network, each node needs a ________.
A) DSL modem
B) network adapter
C) hub
D) router
Answer:  B
Diff: 2
Section Ref:  Basic Network Hardware

20) On a network, a(n) ________ helps prevent data packets from colliding with each other.
A) router
B) hub
C) adapter
D) switch
Answer:  D
Diff: 2
Section Ref:  Basic Network Hardware
21) Sophisticated networks generally use which of the following hardware devices to ease the flow of data through the network?
A) Routers and switches
B) USB ports
C) Firewalls
D) Firmware
Answer:  A
Diff: 2
Section Ref:  Basic Network Hardware

22) To transfer data packets between two or more networks, a ________ is used. 
A) router
B) hub
C) firewall
D) switch
Answer:  A
Diff: 2
Section Ref:  Basic Network Hardware

23) Data are sent through a network in bundles called ________.
A) packages
B) pouches
C) packets
D) nodes
Answer:  C
Diff: 2
Section Ref:  Basic Network Hardware

24) All of the following operating systems support P2P networking EXCEPT ________.
A) Windows
B) OS X
C) Unix
D) Linux
Answer:  C
Diff: 2
Section Ref:  Network Software

25) Client/server networks are controlled by a central server that runs specialized software called a(n) ________.
A) information management system (ISM)
B) network operating system (NOS)
C) digital subscriber line (DSL)
D) service set identifier (SSID)
Answer:  B
Diff: 2
Section Ref:  Network Software
26) Which of the following is NOT a wired broadband Internet connection option?
A) Cable
B) Dial-up
C) DSL
D) Fiber-optic
Answer:  B
Diff: 3
Section Ref:  Wired Broadband Internet Connections

27) A(n) ________ device facilitates file sharing and data backup.
A) NAS
B) WAN
C) UTP
D) NOS
Answer:  A
Diff: 2
Section Ref:  Network-Attached Storage Devices

28) Using a network without the network owner's permission is known as ________.
A) hijacking
B) spamming
C) piggybacking
D) phishing
Answer:  C
Diff: 2
Section Ref:  Securing Wireless Networks

29) All of the following are extra precautions you can take to secure a wireless network EXCEPT ________.
A) change your network name (SSID)
B) enable SSID broadcast
C) turn on security protocols
D) create a passphrase
Answer:  B
Diff: 3
Section Ref:  Securing Wireless Networks

30) The unique number assigned to a network adapter by the manufacturer is referred to as the ________ address.
A) MAC
B) IP
C) SSID
D) network
Answer:  A
Diff: 2
Section Ref:  Securing Wireless Networks

31) The term network ________ refers to the design of a network.
Answer: 	architecture
design
Diff: 1
Section Ref:  Network Architectures
32) A(n) ________ network is one where each computer can communicate directly with the others, rather than having a separate device exercise central control over the entire network.
Answer: 	peer-to-peer
P2P
Diff: 2
Section Ref:  Network Architectures Defined by Levels of Administration

33) A network in which the nodes are located within a computer lab is called a(n) ________.
Answer: 	LAN
local area network
Diff: 1
Section Ref:  Network Architectures Defined by Distance

34) A network used to communicate among devices close to one person is called a(n) ________.
Answer: 	PAN
personal area network
Diff: 1
Section Ref:  Network Architectures Defined by Distance

35) Many cities in the United States now provide a(n) ________ area network to allow Internet access to residents and tourists.
Answer:  metropolitan
Diff: 2
Section Ref:  Network Architectures Defined by Distance

36) ________ cable is composed of four pairs of wires that are twisted around each other to reduce electrical interference.
Answer: 	Unshielded twisted-pair
UTP
Diff: 2
Section Ref:  Transmission Media

37) ________ cable consists of a single copper wire surrounded by layers of plastic and is used to connect cable TV.
Answer:  Coaxial
Diff: 2
Section Ref:  Transmission Media

38) The capability of current devices to use earlier standards is known as ________.
Answer:  backward compatibility
Diff: 2
Section Ref:  Ethernet Protocols

39) ________ are devices that transfer packets of data between two or more networks.
Answer:  Routers
Diff: 2
Section Ref:  Basic Network Hardware
40) A(n) ________ is a device that receives data packets and sends them to their intended nodes while preventing data collisions.
Answer:  switch
Diff: 2
Section Ref:  Basic Network Hardware

41) The server on a client/server network has specialized ________ software installed.
Answer: 	network operating system
NOS
Diff: 2
Section Ref:  Network Software

42) ________ is often referred to as "high-speed Internet."
Answer:  Broadband
Diff: 2
Section Ref:  Wired Broadband Internet Connections

43) DSL uses ________ cable.
Answer:  twisted-pair
Diff: 3
Section Ref:  Wired Broadband Internet Connections

44) A(n) ________ network uses radio waves as its transmission medium.
Answer:  wireless
Diff: 1
Section Ref:  Wired Broadband Internet Connections


45) Storing files on the ________ avoids having to save them on multiple devices.
Answer:  cloud
Diff: 2
Section Ref:  Trends in IT: Where Should You Store Your Files? The Cloud is Calling!

46) In terms of networking, NOS stands for ________.
Answer:  network operating system
Diff: 2
Section Ref:  Network Software

47) A(n) ________ network is set up near a wireless network and has a sound-alike name to lure unsuspecting web surfers.
Answer: 	evil twin
"evil twin"
Diff: 2
Section Ref:  Connecting to Wireless Networks on the Road? Beware of "Evil Twins"!

48) Public places where you can wirelessly connect to the Internet are known as ________.
Answer: 	hotspots
WiFi hotspots
Wi-Fi hotspots
wireless hotspots
Diff: 2
Section Ref:  Wireless Internet Access
49) Someone who breaks into computer systems to create mischief or steal information is a(n) ________.
Answer:  hacker
Diff: 1
Section Ref:  Securing Wireless Networks

50) When using a wireless connection, ________ translates data so that it is protected.
Answer:  encryption
Diff: 2
Section Ref:  Securing Wireless Networks

51) SSID stands for ________.
Answer: 	service set identifier
service set ID
Diff: 3
Section Ref:  Securing Wireless Networks


52) All wireless networks have their own name, referred to as the ________, which is used to identify the network.
Answer: 	service set identifier
SSID
service set ID
Diff: 3
Section Ref:  Securing Wireless Networks

53) WEP stands for ________.
Answer:  wired equivalent privacy
Diff: 3
Section Ref:  Securing Wireless Networks

54) WPA stands for ________.
Answer: 	Wi-Fi protected access
WiFi Protected access
Diff: 3
Section Ref:  Securing Wireless Networks

55) ________ refers to connecting to a wireless connection without the permission of the owner.
Answer:  Piggybacking
Diff: 2
Section Ref:  Securing Wireless Networks

56) A printer connected to a wireless network is considered to be a node on that network.
Answer:  TRUE
Diff: 1
Section Ref:  Networking Fundamentals

57) Sharing files is a benefit of a network.
Answer:  TRUE
Diff: 1
Section Ref:  Networking Fundamentals
58) In a peer-to-peer network, one computer acts as the central computer.
Answer:  FALSE
Diff: 1
Section Ref:  Network Architectures Defined by Levels of Administration

59) P2P networks are most commonly used in home networks.
Answer:  TRUE
Diff: 1
Section Ref:  Network Architectures Defined by Levels of Administration


60) The Internet is a WAN.
Answer:  TRUE
Diff: 1
Section Ref:  Network Architectures Defined by Distance

61) Current wired Ethernet networks in the United States are based on the IEEE 802.11ac standard.
Answer:  FALSE
Diff: 3
Section Ref:  Ethernet Protocols

62) Ethernet networks are always connected using twisted-pair cable technology. 
Answer:  FALSE
Diff: 2
Section Ref:  Transmission Media

63) Wireless network connections are slower than wired broadband connections.
Answer:  TRUE
Diff: 2
Section Ref:  Transmission Media

64) The most popular transmission media option for wired Ethernet networks is UTP cable.
Answer:  TRUE
Diff: 2
Section Ref:  Transmission Media

65) Most computers today come with Ethernet adapters already installed. 
Answer:  TRUE
Diff: 2
Section Ref:  Basic Network Hardware

66) A router acts like a traffic signal on a network.
Answer:  FALSE
Diff: 2
Section Ref:  Basic Network Hardware

67) A P2P network needs network operating system software installed on every node. 
Answer:  FALSE
Diff: 2
Section Ref:  Network Software
68) Wireless networks are more vulnerable to attack than wired networks.
Answer:  TRUE
Diff: 2
Section Ref:  Securing Wireless Networks


69) WEP is a stronger form of security than WPA.
Answer:  FALSE
Diff: 2
Section Ref:  Securing Wireless Networks

70) Limiting your signal range does not help increase wireless network security.
Answer:  FALSE
Diff: 1
Section Ref:  Securing Wireless Networks

71) Match each of the following network types to its definition:
I.	HAN
II.	MAN
III.	LAN
IV.	PAN
V.	WAN

A.	confined to a small geographic location beyond the home
B.	services a residence
C.	used to communicate among devices near an individual
D.	covers a city
E.	a network that covers a great distance
Answer:  B, D, A, C, E
Diff: 1
Section Ref:  Network Architectures Defined by Distance

72) Match each of the following terms to its definition:
I.	fiber-optic
II.	twisted pair
III.	coaxial cable
IV.	peer-to-peer
V.	client/server

A.	single copper wire surrounded by layers of plastic
B.	made up of plastic or glass and transmits data at extremely fast speeds
C.	each node can communicate directly with every other node on the network
D.	made up of copper wires
E.	central computer provides information and resources to other computers
Answer:  B, D, A, C, E
Diff: 2
Section Ref:  Multiple locations in the chapter

73) Match each of the following terms to its definition:
I.	server
II.	client
III.	network
IV.	piggyback
V.	node

A.	two or more computers connected together via software and hardware so they can communicate
B.	a computer, peripheral, or communication device on a network 
C.	computer on which users accomplish specific tasks and make specific requests 
D.	provides information and resources to other computers on a network 
E.	unauthorized connection to a wireless network 
Answer:  D, C, A, E, B
Diff: 3
Section Ref:  Multiple locations in the chapter

74) Match each of the following terms to its definition:
I.	throughput
II.	packet
III.	firmware
IV.	firewall
V.	bandwidth

A.	maximum speed at which data can be transmitted
B.	the actual speed of data transfer that is achieved on a network
C.	the format in which data is sent over transmission media
D.	hardware or software for protecting computers from hackers
E.	instructions in read-only memory
Answer:  B, C, E, D, A
Diff: 2
Section Ref:  Multiple locations in the chapter
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75) Match each of the following terms to its definition:
I.	NOS
II.	broadband
III.	router
IV.	switch
V.	NIC

A.	directs data traffic between networks
B.	handles data traffic between nodes on the same network
C.	software used to set up and manage a network
D.	connects a node to a network
E.	high-speed Internet connection
Answer:  C, E, A, B, D
Diff: 3
Section Ref:  Multiple locations in the chapter

